1. **SCOPE OF WORK**

Provide on-call professional safety rubber surfacing installation service. Services shall include resealing or replacement of failed, one or two-layer poured in place rubber surfacing. Materials shall be highly durable and of commercial quality; any substitute replacement materials shall be appropriate to the specific park, site, and operating conditions.

This is an indefinite quantity contract with no guarantee services will be required. The County does not guarantee a minimum or maximum dollar amount to be expended on any contract(s). All work performed shall be in strict compliance with the latest codes, standards, and practices and in accordance with Federal, State, and Local laws.

1. **CONTRACTOR RESPONSIBILITIES**

Contractor shall:

* 1. Visit each site to verify and provide the approximate square footage required to complete the project.
	2. Provide all labor, fuel, materials, equipment, storage, supplies, and incidental costs necessary to complete the tasks.
	3. Provide for skilled, qualified, and English-speaking staff with a cell phone in good working order.
	4. Provide a neat and clean in appearance dress code for Contractor’s employees that consists of a shirt with company name, pants, and work shoes/boots.
	5. Project a professional image, deal effectively with the public, and discharge duties in a courteous and efficient manner.
	6. Maintain the rubber surface areas in a clean, attractive, and uniform manner which will reflect favorably upon the County and the Contractor.
	7. Work shall be performed at a time that minimizes disturbance or interference to visitor activities.
1. **COUNTY RESPONSIBILITIES**
	1. Reserves the right to award to one or more vendors.
	2. Reserves the right to add or remove services in conjunction with the County’s needs.
2. **DELIVERY REQUIREMENTS AND ACCEPTANCE**

FOB-Destination.

1. **ORDER OF OPERATION**
	1. Site preparation shall include, but is not limited to, removal and replacement of play structures, scribing, cutting, removal, and disposal of the existing deteriorated rubber surface.
	2. Project spoils shall be properly disposed of offsite at the Contractor’s expense.
	3. Concrete substrate preparation shall include, but is not limited to, sand blasting or other associated substrate preparation.
	4. Provide for proper completion and functioning of the proposed resurfacing installation in accordance with product manufacturer specifications and generally accepted industry installation standards.
	5. Thicknesses will vary to meet specific playground equipment fall heights; existing poured in place surfaces range from ½”, 1”, 1 ½”, to 2” thick.
	6. Colors and designs of surfacing shall match existing, or alternates be proposed for review and approval by the County prior to installation.
	7. Mix proportions shall be per the manufacturers recommendations for the system used.
	8. Rubber surface sealer of Aliphatic Polyurethane Binder shall be applied per manufacturer’s specifications.
	9. Reinstall play structures, as required.
2. **PRODUCT REQUIREMENTS**
	1. Products shall be highly durable, low maintenance, commercial quality, and substitute replacements shall be appropriate to park replacement, site, and operating conditions.
	2. Aesthetically pleasing.
	3. UV color stable.
	4. Safe and resilient construction.
	5. Stable, slip resistant surfaces comfortable for bare feet.
	6. Vandal resistant.
	7. No initial binder ambering.
	8. Must meet all applicable ASTM standards.
	9. ADA complaint, uniform, stable accessibility.
	10. Fire and Chemical resistant.
	11. Bacteria, mildew, and algae resistant.
	12. Allows for expansion and contraction.
3. **WARRANTY REQUIREMENTS**
	1. Three (3) year warranty on repair and replacement poured in place rubber.
	2. Correct all apparent deficiencies within two (2) calendar day of any work that fails to conform to the specifications.

[*The remainder of this page intentionally left blank*]