1. **SCOPE OF SERVICES**

Provide for the one-time purchase of commercial-grade fitness equipment. The equipment shall be new, in accordance with the minimum specifications, and include a minimum of one-year commercial use warranty. Manufacturer and models specified is to establish a minimum level of acceptable quality. Exception items shall be of equal or greater precision equipment.

This is an indefinite quantity contract with no guarantee of a minimum or maximum purchase value. Equipment purchases shall be made on an as needed basis in conjunction with the County’s needs. Equipment shall be manufactured in strict conformance to industry and safety standards and in accordance with all Federal, State, or Local laws and regulations.

1. **CONTRACTOR’S RESPONSIBILITIES**

The Contractor:

* 1. Shall provide commercial grade fitness equipment.
  2. Shall provide all equipment and tools necessary to deliver.
  3. Shall provide descriptive literature detailing the specifications for each bid item.
  4. Shall provide additional equipment not specified herein and/or services in conjunction with the County’s needs.

1. **COUNTY RESPONSIBILITIES**

The County:

* 1. Reserves the right to purchase individual items as needed.
  2. Reserves the right to add or delete equipment products in conjunction with the County’s needs.
  3. Reserves the right to purchase ancillary items not listed for purchased equipment.
  4. Reserves the right to reject or approve exception items.

1. **DELIVERY REQUIREMENTS AND ACCEPTANCE**
   1. Delivery to zip code 34788 shall be included in the bid price.
   2. Delivery shall be FOB destination.
2. **ITEMS & SPECIFICATIONS**
   1. **Barbel Power Bar** **– Qty 28**
      1. High-grade steel alloy or equivalent
      2. Tensile strength 200,000 PSI
      3. Load capacity 1,500lbs
      4. Center knurl and dual knurl markings
      5. Durable and corrosion-protective finish
      6. Bar shaft diameter approx. 29mm
      7. Bar weight approx. 20kg (44lbs)
      8. Full bar length of approx. 86.5 inches
      9. Loadable sleeve of approx. 16.25 inches
      10. Compliant with International powerlifting standards including International Powerlifting Federation (IPF) regulations for competition use
   2. **Adjustable Bench – Qty 28**
      1. Heavy duty 11-gauge steel material
      2. Weight capacity 700lbs
      3. Length at least 49 inches
      4. Scratch and corrosion-resistant coated steel frame
      5. High-density foam padding with grippy vinyl cover
      6. Adjustable back pad, minimum 7 positions ranging from 0 degree (flat) to 85 degree (near upright)
      7. Adjustment seat, minimum3 positions including flat and incline settings
      8. Ladder-style adjustment mechanism
      9. Approx. 85lbs or heavier
      10. Built-in handle and rear-mounted wheels for portability
      11. Compliant with ASTM International safety standards
      12. Able to be stored upright
   3. **Hi-Temp Bumper Plates (1 set = 2 pairs of 45lb and 1 pair each of 25lb and 10lb. Total 250lbs per set – Qty 28 sets**
      1. Constructed from durable, shock-absorbent, vulcanized rubber or equivalent
      2. Bonded stainless steel or zin-coated, rust-resistant insert hub. Designed for a secure fit on standard Olympic barbell sleeve (50mm diameter)
      3. Complies with International Weightlifting Federation (IWF) standards for dimension and performance
   4. **Kettlebells (1 set = 1 each 16kg, 24kg and 28kg) – Qty 28 sets**
      1. Solid cast iron or steel with powder-coated finish. No welds, single piece of cast iron.
      2. Wide, flat machined bottoms
   5. **EZ Curl Bar – Qty 28**
      1. High-strength steel material
      2. Corrosion-resistant coating (zinc or equivalent)
      3. Chrome-plated, 6.5 inches loadable sleeves
      4. Medium knurl texture with an EZ-curl shape
      5. Weight approx. 30lbs (13.6kg)
      6. Length approx. 47 inches
      7. Shaft Diameter approx. 28mm
      8. Designed for compatibility with Olympic weight plates
      9. Meets industry standards for home/commercial gym use
3. **WARRANTY REQUIREMENTS**
   1. A minimum of one-year commercial use warranty unless otherwise specified.

[*The remainder of this page intentionally left blank*]